( TL19E20A20326437601FEAT00 )

Low Fuel Indicator Test

1. Do the gauge self-diagnostic test.
   - If the low fuel indicator flashes, go to Step 2 .
   - If the low fuel indicator does not flash, replace the gauge control module.

1. Check for body electrical system DTCs.
   - If any DTCs are indicated, do the indicated DTC's troubleshooting.
   - If no DTCs are indicated, go to Step 3 .

1. Do the fuel gauge sending unit test.