( TL19E00J18526234603KBAT00 )

Rear Inner Fender Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the rear bumper and the body.

1. Remove the screws (A) securing the rear inner fender (B) and the rear bumper (C), and remove the screw (D) securing the rear inner fender and the body.
   Left side on R20A3 engine model: Remove the clips (E) securing the rear inner fender and the side rear undercover.
   NOTE: To remove the clips, pry the inner clip up at the edge near the line (F) on its head.