( TL19E1PE10411412282KCAT00 )

A/T Shift Lever Installation

1. Install and tighten the nut (A) on the shift cable end.

1. Remove the 6.0 mm (0.24 in.) pin (B) that was installed to hold the shift lever.

1. Turn the ignition switch to ON (II). Move the shift lever to each position, and check that the A/T gear position indicator follows the transmission range switch.

1. Shift the shift lever to P, and check that the shift lock works properly. Push the shift lock release, and check that the shift lever releases, and also check that the shift lever locks when it is shifted back to P.

1. Install the center console.