( TL19E00F00000057161KAAT00 )

Steering Wheel Removal

SRS components are located in this area. Review the SRS component locations, and the precautions and procedures before doing repairs or service.

1. Do the battery terminal disconnection procedure.

1. Align the front wheels straight ahead, then remove the driver's airbag from the steering wheel.

1. Disconnect the cable reel subharness connector (A).

1. Loosen the steering wheel bolt (B).