( TL19E00F18100000000FAAT02 )

EPS Symptom Troubleshooting - EPS indicator does not go off, and no DTCs are stored

EPS indicator does not go off, and no DTCs are stored
NOTE: Check for gauge DTCs with the HDS. If gauge DTCs are stored, troubleshoot those DTCs first.

1. Turn the ignition switch to LOCK (0).

1. Check the No. 6 (7.5 A) fuse in the driver's under-dash fuse/relay box.

Is the fuse blown?

YES | - | Go to Step 3 .
NO | - | Reinstall the checked fuse, then go to Step 5 .

1. Disconnect the EPS control unit connector D (28P).

1. Check for continuity between EPS control unit connector D (28P) terminal No. 16 and body ground.

Is there continuity?

YES | - | Repair short to body ground in the wire between the EPS control unit and the No. 6 (7.5 A) fuse in the driver's under-dash fuse/relay box.■
NO | - | Install a new No. 6 (7.5 A) fuse in the driver's under-dash fuse/relay box, then go to Step 6 .

1. Disconnect the EPS control unit connector D (28P).

1. Turn the ignition switch to ON (II).