( TL19E00J46127000000KDAT00 )

Front Seat Removal/Installation

1. Lift up the front seat, then detach the harness clip(s) (A), and disconnect the side airbag connector (B), the seat wire harness connector (C) on the seat with seat heater, and the seat belt buckle switch connector (D). On the passenger's seat, disconnect the passenger's seat sitting switch connector (E) on the seat without seat heater, and if equipped, the OPDS unit harness connector (F).

1. Remove the head restraint.

1. With the help of an assistant, carefully remove the front seat through the front door opening.

Driver's seat (8-way power seat)
Driver's seat (manual seat/manual height adjustable seat without seat heater)
Driver's seat (manual height adjustable seat with seat heater)
Passenger's seat without OPDS (8-way power seat)
Passenger's seat without OPDS (manual seat without seat heater)
Passenger's seat without OPDS (manual seat with seat heater)
Passenger's seat with OPDS on RHD model (8-way power seat)
Passenger's seat with OPDS on RHD model (manual seat without seat heater)