( TL19E1PE10410744859FAAT00 )

A/T Paddle Shifter - (Downshift Switch) Illumination Circuit Troubleshooting

1. Check for continuity cable reel 20P connector terminal No. 9 and gauge control module connector terminal No. 2.

Is there continuity?

YES | - | Check the illumination control circuit in the gauge control module self-diagnostic function. ■
NO | - | Repair open in the wire between cable reel 20P connector terminal No. 9 and the gauge control module.■