( TL19E00J10300000000FAAT05 )

Audio System Symptom Troubleshooting - No sound is heard from the speaker(s) (display is normal) (with premium audio system)

1. Check for continuity between stereo amplifier connector B (18P) according to the table.

   Speaker | Stereo amplifier terminal | Wire color
   --- | --- | ---
   Left front door speaker, Left front tweeter | A16 (+) | BLK
   A7 (−) | BLU
   Right front door speaker, Right front tweeter | A15 (+) | RED
   A6 (−) | GRN
   Left rear door speaker | A13 (+) | WHT
   A4 (−) | GRN
   Right rear door speaker | A12 (+) | RED
   A3 (−) | BLU
   Front center speaker | A11 (+) | YEL
   A2 (−) | BLU
   Subwoofer | A10 (+) | GRY
   A1 (−) | LT BLU
   Left rear speaker | A17 (+) | YEL
   A8 (−) | BRN
   Right rear speaker | A14 (+) | BLU [PNK]
   A5 (−) | ORN [BRN]

   [ ]: | RHD model

Is there continuity?

YES | - | Go to Step 14 .
NO | - | Repair open in the wire between the stereo amplifier and the speaker or door speaker network control unit.■

1. Disconnect the jumper wire.