( TL19E00F00000057111KDAT00 )

Steering Gearbox Removal and Installation

1. Align the front subframe using the 15.7 mm end of the subframe alignment pin. Vertically install the subframe alignment pin, and align the right-rear corner of the front subframe and vehicle frame holes, then loosely tighten the subframe mounting bolt (A) unit the front subframe contacts the body frame.

1. Loosely tighten the left-rear subframe mounting bolt with the same procedure as right-rear using the subframe alignment pin.