( TL19E00K77C000Y2626FAAT00 )

DTC Troubleshooting: B2626

DTC B2626:
Left Front Center Parking Sensor Malfunction

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Check for DTCs with the HDS.

Is DTC B2626 indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Turn the ignition switch to LOCK (0).

1. Swap the left front center parking sensor and the left front corner parking sensor.

1. Turn the ignition switch to ON (II).

1. Check for DTCs with the HDS.

Is DTC B2626 indicated?

YES | - | Go to Step 8 .
NO | - | Replace the left front center parking sensor.■

1. Turn the ignition switch to LOCK (0).

1. Disconnect the 6P connector from the left front center parking sensor.

1. Turn the ignition switch to ON (II).

1. Measure the voltage between the left front center parking sensor 6P connector No. 6 terminal and body ground.

Is there about 8 V?

YES | - | Go to Step 12 .
NO | - | Go to Step 19 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect the 6P connector from the left front corner parking sensor.