( TL19E00H46400055413KBAT00 )

Side Impact Sensor (Second) Replacement

Removal

1. Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Disconnect the appropriate side curtain airbag 2P connector.

1. Remove the seat side bolster.

1. Disconnect the SRS floor wire harness 2P connector (A) from the side impact sensor (second) (B).

1. Using a TORX T30 bit, remove the TORX bolt (C) then remove the side impact sensor (second).