( TL19E00E16226622502KBAT00 )

Driveshaft Dynamic Damper Replacement

1. Adjust the specified distance (A) between the outboard joint side and the dynamic damper edge.
   NOTE: Check the type of dynamic damper at its shape.

Model | Left/Right Driveshaft | Dynamic Damper Type | Specified Distance (A)
--- | --- | --- | ---
R20A3 engine model | M/T | Left | 2 | 295.5−300.5 mm (11.63−11.83 in.)
Right | 1
A/T | Left | 1 | 295.5−300.5 mm (11.63−11.83 in.)
Right | 1
K24Z3 engine model | M/T | Left | 2 | 295.5−300.5 mm (11.63−11.83 in.)
Right | 1
A/T | Left | 1 | 298.5−303.5 mm (11.75−11.95 in.)
Right | 2 | 292.5−297.5 mm (11.52−11.71 in.)

1. Install the dynamic damper band.

1. Install the inboard joint.

Dynamic damper type 1
Dynamic damper type 2