( TL19E00J32100017101FHAT00 )

Combination Light Switch Test/Replacement

1. Inspect the connector terminals to be sure they are all making good contact.
   - If the terminals are bent, loose or corroded, repair them as necessary, and recheck the system.
   - If the terminals look OK, check for continuity between the terminals in each switch position according to the tables.

   - | If the continuity is not as specified, replace the switch.