( TL19E00K761000N1302FAAT00 )

DTC Troubleshooting: 1302

DTC 1302:
GPS Receiver Error 1
NOTE:

- Check the vehicle battery condition first.
- Before you troubleshoot, make sure to follow the general troubleshooting information.
- Make sure the vehicle is parked outside and away from buildings.
- Aftermarket electronic devices located near the navigation unit or GPS antenna can potentially interfere with the operation of the navigation system.

1. Clear the hard error code.

1. Turn the ignition switch to LOCK (0), and then back to ON (II).

1. Check for the hard error code.

Is DTC 1302 indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Turn the ignition switch to LOCK (0).

1. Check for poor connections or loose terminals at the navigation unit connector E (2P).

1. Clear the hard error code.

1. Turn the ignition switch to LOCK (0), and then back to ON (II).

1. Check for the hard error code.

Is DTC 1302 indicated?

YES | - | Replace the GPS Antenna. ■
NO | - | Repair poor connections or loose terminals at the navigation unit, and then reconnect all connectors.■