( TL19E00J22100030053KBAT00 )

Gauge Control Module Replacement

NOTE: Before replacing the gauge control module, retrieve the ODO value and the maintenance minder information from the gauge control module with the HDS.

1. Remove the driver's dashboard undercover, then remove the dashboard lower cover.

1. Remove the two bolts from under the dashboard, then pull the gauge control module (A) out carefully.

1. Disconnect the 32P connector (B) from the gauge control module.

1. Install the gauge control module in the reverse order of removal.

1. Write the ODO value and maintenance minder information to the new gauge control module.

NOTE: Before replacing the gauge control module, retrieve the ODO value and the maintenance minder information from the gauge control module with the HDS.

1. Remove the driver's dashboard undercover, then remove the dashboard lower cover.

1. Remove the two bolts from under the dashboard, then pull the gauge control module (A) out carefully.

1. Disconnect the 32P connector (B) from the gauge control module.

1. Install the gauge control module in the reverse order of removal.

1. Write the ODO value and maintenance minder information to the new gauge control module.