( TL19E00H46400000000AAAT00 )

SRS Precautions and Procedures

- After a collision where a front airbag, side airbags, side curtain airbags, seat belt tensioner, or seat belt outer lap tensioner deployed, go to Component Replacement/Inspection after Deployment. After a collision where the airbags or the side airbags did not deploy, inspect for any damage or any deformation on the SRS unit, front impact sensors, and side impact sensors. Replace all damaged parts.

- Do not disassemble the SRS unit, front impact sensors, and side impact sensors.
- Be sure the SRS unit, front impact sensors, and side impact sensors are installed securely with the mounting bolts torqued to 9.8 N·m (1.0 kgf·m, 7.2 lbf·ft) whenever you remove or replace the SRS unit, rear safing sensor, all impact sensors, always install the components with new bolts.
- Do not spill water or oil on the SRS unit or the side impact sensors.