( TL19E00K761000N1101FAAT00 )

DTC Troubleshooting: 1101

DTC 1101:
Media Bus Send Error
NOTE:

- Check the vehicle battery condition first.
- Before you troubleshoot, make sure to follow the general troubleshooting information.
- When Soft Error of the Hard Error/ Soft Error in the Error History menu is displayed in yellow, select Save first before selecting Clear.

1. Clear hard error code.

1. Turn the ignition switch to LOCK (0), and then back to ON (II).

1. Check for the hard error code.

Is DTC 1101 indicated?

YES | - | Replace the navigation unit. ■
NO | - | Intermittent failure, the system is OK at this time.■