( TL19E00J10300000000CAAT10 )

Audio Unit Connector for Inputs and Outputs
With Premium Audio System (Without Navigation System)
AUDIO UNIT CONNECTOR A (24P)
Audio Unit Connector A (24P)

Cavity | Wire | Connects to
--- | --- | ---
A1 | RED | Dash lights brightness controller (ILL BULB)
A3 | LT BLU | Data link connector (DLC) (K-LINE)
A4 | YEL | Passenger's multiplex integrated control unit (SCTY)
A5 | BRN | Audio remote switch ground (REMOTE GND)
A12 | BLK | Ground (G401) (MAIN GND)
A13 | GRY | Light-on signal (ILL+)
A14 | PUR | Audio power supply (ACC)
A16 | PNK | Audio remote switch (REMOTE)
A17 | WHT | Stereo amplifier (SWD +B)
A18 | GRN | Stereo amplifier (FR PRE−)
A19 | BLK | Stereo amplifier (FR PRE+)
A21 | GRY * | Stereo amplifier (SH FR-FL GND)
A22 | WHT | Stereo amplifier (FL PRE−)
A23 | RED | Stereo amplifier (FL PRE+)
A24 | WHT | Constant power (+B)

*: | The shielded wires have a heat-shrink tube insulating the outside of the wire. The color of the insulating tube, typically black or dark gray, may not match the color of the wire shown on the circuit diagram.

AUDIO UNIT CONNECTOR B (20P)
Audio Unit Connector B (20P)

Cavity | Wire | Connects to
--- | --- | ---
B3 | BLK | Auxiliary jack assembly (AUX SIG GND)
B4 | GRY * | Auxiliary jack assembly (AUX SH GND)
B5 | YEL | Auxiliary jack assembly (AUX GND)
B6 | RED | Center display unit (DUET TX (UART))
B7 | GRN | Center display unit (DUET RX (UART))
B8 | BLU | B-CAN bus communication (B-CAN L)
B9 | RED | Hands free telephone control unit (TELM SIG−)
B10 | GRY * | Hands free telephone control unit (TELM SIG SH)
B13 | RED | Auxiliary jack assembly (AUX LCH)
B14 | WHT | Auxiliary jack assembly (AUX RCH)
B15 | GRY | Auxiliary jack assembly (AUX DET)
B16 | GRY * | Center display unit (SH DUET GND)
B17 | BLU | Center display unit (DUET CONT)
B18 | PNK | B-CAN bus communication (B-CAN H)
B19 | GRN | Hands free telephone control unit (TELM SIG+)
B20 | LT GRN | Hands free telephone control unit (HFT MUTE)

*: | The shielded wires have a heat-shrink tube insulating the outside of the wire. The color of the insulating tube, typically black or dark gray, may not match the color of the wire shown on the circuit diagram.

AUDIO UNIT CONNECTOR C (12P)
Audio Unit Connector C (12P)

Cavity | Wire | Connects to
--- | --- | ---
C1 | RED | Stereo amplifier (ELS DATA−)
C2 | GRN | Stereo amplifier (ELS DATA+)
C7 | GRY * | Stereo amplifier (SH ELS GND)

*: | The shielded wires have a heat-shrink tube insulating the outside of the wire. The color of the insulating tube, typically black or dark gray, may not match the color of the wire shown on the circuit diagram.

AUDIO UNIT CONNECTOR D (14P)
Audio Unit Connector D (14P)

Cavity | Wire | Connects to
--- | --- | ---
D1 | WHT | USB adapter unit (+B)
D2 | LT BLU | USB adapter unit (SYS ON)
D3 | GRY * | USB adapter unit (GA-NET BUS SH)
D4 | GRY * | USB adapter unit (AUDIO SH)
D5 | GRN | USB adapter unit (AUDIO R+)
D6 | BLK | USB adapter unit (AUDIO L+)
D9 | RED | USB adapter unit (GA-NET BUS+)
D10 | GRN | USB adapter unit (GA-NET BUS−)
D11 | BLK | USB adapter unit (GND)
D13 | WHT | USB adapter unit (AUDIO R−)
D14 | RED | USB adapter unit (AUDIO L−)

*: | The shielded wires have a heat-shrink tube insulating the outside of the wire. The color of the insulating tube, typically black or dark gray, may not match the color of the wire shown on the circuit diagram.

AUDIO UNIT CONNECTOR E (5P)
Audio Unit Connector E (5P)

Cavity | Wire | Connects to
--- | --- | ---
E1 | ——— | AM/FM amplifier (RF SUB IN)
E2 | ——— | AM/FM amplifier (RF SUB SH)
E3 | ——— | AM/FM amplifier (RF MAIN IN)
E4 | ——— | AM/FM amplifier (RF MAIN SH)
E5 | ——— | AM/FM amplifier (ANT +B)