( TL19E00H46400000000AAAT00 )

SRS Precautions and Procedures

- Be sure to install the harness wires so they do not get pinched or interfere with other parts.

- Make sure all SRS ground locations are clean, and grounds are securely fastened for optimum metal-to-metal contact. Poor grounds can cause intermittent problems that are difficult to diagnose.
- Do not use any silicone based cleaners or lubricants on any SRS connectors or terminals.