( TL19E00J26200016101KBAT00 )

Carpet Replacement

1. Release the Velcro fastener (A) (for some models), and release the carpet (B) from the hooks (C) of both rear heater ducts. Remove the clips (D). Detach the clips (E) fastening the carpet to both door sill areas:
   - Replace the clips (E) with new ones.
   - LHD model is shown; RHD model is symmetrical.

1. Pull the carpet out from under the dashboard, then remove the carpet. Pull the seat harnesses (F) out through the holes in the carpet. LHD model is shown; RHD model is similar.

1. Install the carpet in the reverse order of removal, and note these items:
   - Take care not to damage, wrinkle or twist the carpet.
   - Make sure the seat harnesses are routed correctly.
   - Slip the holes in the carpet over the rear heater ducts.
   - If the clips fastening the carpet to the floor are damaged or stress-whitened, replace them with new ones.
   - Replace the clips fastening the carpet to both door sill areas with new ones.
   - Push the Velcro fastener and the clips into place securely.
   - Do the battery terminal reconnection procedure.
   - If necessary, adjust the parking brake cable.
   - Push the accelerator pedal hook into place securely, and after installing, make sure the accelerator pedal does not come the floor by pulling it back.