( TL19E1PE10410744859FAAT00 )

A/T Paddle Shifter - (Downshift Switch) Illumination Circuit Troubleshooting

1. Check for continuity between paddle shifter − (downshift switch) connector terminals No. 1 and No. 2.

Is there continuity?

YES | - | Replace the cable reel subharness.■
NO | - | Replace the paddle shifter − (downshift switch). ■

1. Remove the cable reel.

1. Turn the ignition switch to ON (II), and turn the combination light switch to the PARKING (SMALL) position.