( TL19E00K75100081090FAAT00 )

DTC Troubleshooting: 9, 15

1. Check for continuity between LKAS control unit 26P connector No. 25 terminal and gauge control module 32P connector No. 21 terminal.

Is there continuity?

YES | - | Check for loose terminals in the gauge control module connector, and repair if necessary. If all connections are OK, replace the gauge control module. ■
NO | - | Repair an open in the wire between the LKAS control unit and the branch of the F-CAN line (CANL).■