( TL19E00J34600000000CAAT00 )

Wiper/Washer
The driver's MICU controls the wiper based upon the input signals from each switch.

| Input | Output
--- | --- | ---

Driver's MICU

IG1 power supply
Brake pedal position switch
Transmission range switch P position (A/T)
Wiper switch (INT & LO)
Wiper switch (HI & LO)
Wiper switch (MIST)
Wiper switch (As)
Wiper switch intermittent dwell time controller

Wiper intermittent relay circuit
Wiper motor high/low relay circuit

B-CAN | Parking brake signal (A/T) IG1 meter signal (A/T) Vehicle speed signal Washer signal | Wiper messages