( TL19E1AE34116317041MBAT00 )

Clutch Pedal, Clutch Pedal Position Switch, and Clutch Switch (SIL) Adjustment

1. Tighten the clutch pushrod locknut (A).

1. With the clutch pedal released, turn in the clutch pedal position switch (B) until it contacts the clutch pedal.

1. Turn to clockwise the clutch pedal position switch an additional 3/4 to 1 turn.

1. Tighten the clutch pedal position switch locknut (C) while holding the clutch pedal position switch.

1. If the vehicle with shift indicator lamp, go to Step 9 . If the vehicle without shift indicator lamp, go to Step 12 .