( TL19E00E16236500000KCAT00 )

Intermediate Shaft Installation

1. Clean the areas where the intermediate shaft contacts the differential thoroughly with solvent or brake cleaner, and dry with compressed air.
   NOTE: Do not wash the rubber parts with solvent.

1. Install a new set ring (A) onto the set ring groove (B) of the intermediate shaft (C).
   NOTE: The illustrations show K24Z3 engine model.

1. Insert the intermediate shaft into the differential correctly.
   NOTE: Insert the intermediate shaft carefully to prevent damaging the oil seal (D).

1. Install the flange bolt (A) and two dowel bolts (B).

1. Install the right driveshaft.

R20A3 engine model
K24Z3 engine model

1. K24Z3 engine model of M/T: Install the CKP sensor cover (A) to the engine block.

1. Refill the transmission with the recommended transmission fluid:
   - Manual transmission
   - Automatic transmission

1. Check the wheel alignment, and adjust it if necessary.

1. Test-drive the vehicle.