( TL19E00K75200081040FAAT00 )

DTC Troubleshooting: 4, 5

1. Check for continuity between LKAS camera 10P connector No. 3 terminal and LKAS control unit 26P connector No. 24 terminal.

Is there continuity?

YES | - | Check for loose terminals in the LKAS camera 10P connector and LKAS control unit 26P connector. If all connections are OK, replace the LKAS camera and LKAS control unit as a set.
NO | - | Repair open in the wire between the LKAS camera and LKAS control unit.■

1. Check for DTCs with the HDS.

Is DTC 7 or 8 indicated?

YES | - | Do the troubleshoot for DTC 7 or 8.■
NO | - | Intermittent failure, the system is OK at this time.■