( TL19E1AE34116317041KBAT00 )

Clutch Pedal Assembly Replacement

NOTE:

- Without cruise control: The adjusting bolt is substituted as clutch pedal position switch.
- Without shift indicator lamp: Exclude the clutch switch (SIL) relation procedure because the switch is not equipped.
- The illustrations show LHD model.

1. Remove the driver's dashboard undercover.

1. Disconnect the clutch pedal position switch connector (A) and the clutch switch (SIL) connector (B).

1. Pry out the lock pin (C), and pull the pedal pin (D) out of the yoke.

1. Remove the master cylinder mounting nuts (E) and the clutch pedal mounting bolt (F).

1. Remove the clutch pedal assembly (G).

1. Remove the clutch pedal position switch (H) and clutch switch (SIL) (I).