( TL19E20A14100022205KDAT00 )

Drive Belt Auto-tensioner Removal/Installation

1. Remove the drive belt auto-tensioner (A).

1. Check for oil leakage from the drive belt auto-tensioner dumper and check for damaged to the dumper rubber (B). If the damage or oil leaks, replace the drive belt auto-tensioner.

1. Install the drive belt auto-tensioner, then do the auto-tensioner air bleeding.

1. Install the water pump pulley.

1. Install the alternator.

1. Install the drive belt.