( TL19E00J4616185367CKBAT00 )

Front Seat Up-down Motor Motor Replacement

1. Install the motor in the reverse order of removal, and note these items:
   - Apply multipurpose grease to the pivot portions of the up-down adjuster and the motor pinion.
   - When installing the front up-down motor (A), adjust the gear (B) to the motor pinion (C) by slightly rotating the brake (D) with a 8 mm hexagonal wrench.
   - Make sure the motor connector is plugged in properly.
   - Check the front seat up-down operation.