( TL19E00J18573426965KBAT00 )

Front Fender Trim Replacement

For Some Models
NOTE:

- Take care not to scratch the front grille cover and the body.
- The left side is shown; the right side is similar.

1. Remove the front grille cover.

1. Remove the front fender trim (A).

   -1. | Remove the clips securing the trim.
   -2. | Pull the trim up, and slide the trim forward to release the hook (B) of the trim from under the front fender (C).

1. Install the trim in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, and replace them with new one.
   - Push the clips into place securely.