( TL19E1PE10400013011KBAT00 )

ATF Cooler Replacement

1. Remove the front bumper.

1. Remove the bolts (A) securing the ATF cooler (B).

1. Remove the ATF cooler hoses (A) from the ATF cooler, then plug the hoses. Replace the ATF cooler.

1. Install the ATF cooler, then remove the plugs from the hose.

1. Slide the ATF cooler hoses with the blue dot end (B) over the ATF cooler lines (C) until the hose end contacts the bulge (D), and secure each hose with the clip (E) at 6−8 mm (0.24−0.31 in.) (F) from the hose end.

1. Secure the ATF cooler with the bolts.

1. Install the front bumper.

1. Check the ATF level.