( TL19E30A14674359528KCAT00 )

Cam Chain Case Oil Seal Installation

Special Tools Required
Driver handle, 15 x 135L
07749-0010000
Bearing driver attachment, 52 x 55 mm
07746-0010400

1. Use the driver handle and the bearing driver attachment to drive a new oil seal squarely into the chain case to the specified installed height.

1. Measure the distance between the chain case surface and the oil seal.

   Oil Seal Installed Height:
   32.4−33.1 mm (1.28−1.30 in.)