( TL19E10D14300014701KBAT00 )

Brake Booster Replacement

1. Remove the brake booster (A) from the engine compartment.
   - Be careful not to damage the booster surfaces and the threads of the booster stud bolts.
   - Be careful not to bend or damage the brake lines.
   NOTE: Use the new brake booster gasket (B) reassembly.

1. Install the brake booster in the reverse order of removal, and note these items:
   - Install the master cylinder after installing the brake booster.
   - Check the brake pedal height and free play after installing the master cylinder, and adjust it if necessary.
   - Bleed the brake system.