( TL19E00F00000057111KDAT00 )

Steering Gearbox Removal and Installation

1. Wipe off any grease contamination from the ball joint tapered section and thread. Reconnect the tie-rod ball joint (A) to the knuckle. Install the nut (B), and tighten it to the specified torque.

1. Install a new cotter pin (C) and bend it as shown.

1. Install the front wheels, then set the wheels in the straight ahead position.
   NOTE: Before installing the wheel, clean the mating surfaces of the brake disc and the inside of the wheel.

1. Center the steering rack within its stroke.