( TL19E20A20326919461FAAT00 )

DLC Circuit Troubleshooting

1. Check for continuity between ECM/PCM connector terminal C36 and body ground.

Is there continuity?

YES | - | Repair short in the wire between the No. 9 FUEL PUMP (20 A) fuse and the ECM/PCM (C36), between the No. 9 FUEL PUMP (20 A) fuse and PGM-FI main relay 2 (FUEL PUMP), or between the No. 9 FUEL PUMP (20 A) fuse and the immobilizer control unit. Also replace the No. 9 FUEL PUMP (20 A) fuse.■
NO | - | Go to Step 51 .

1. Remove the rear seat cushion.

1. Remove the access panel from the floor.

1. Disconnect the fuel pump 4P connector.