( TL19E00R311000K5352YDAT03 )

Front Side Frame/Outrigger Removal

NOTE: This section explains the procedures after removal of all accessories and related parts. For accessories' and related parts' removal procedure, refer to the appropriate Shop Manual.
Mass production body welding position and number (Front side frame)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Mass production body welding position and number (Outrigger and side frame rear end)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Construction

- When removing the front side frame, leave the side frame rear end, the outrigger, and the subframe rear bracket in place.
- Check the side frame rear end, the outrigger, and the subframe rear bracket position for damage. If necessary, replace them as an assembly.