( TL19E20A20323425231FEAT00 )

EVAP Two Way Valve Test

Special Tools Required
Combination gauge kit 20/−100 kPa
07YAJ-0010610
Tube joint adapter
07410-5790503

1. Remove the fuel fill cap.

1. Remove the EVAP two way valve.

1. Disconnect the vapor line from the EVAP two way valve (A). Connect it to the combination gauge kit and tube joint adapter and the vacuum pump (B) as shown.

1. Apply vacuum slowly and continuously while watching the gauge. The valve should open below 1.33 kPa (1.0 mmHg, 0.04 in.Hg).
   - If the vacuum hold below 1.33 kPa (1.0 mmHg, 0.04 in.Hg), go to Step 5 .
   - If the vacuum doesn't hold, replace the EVAP two way valve.

1. Move the vacuum pump from the vacuum fitting to the pressure fitting (A) as shown.

1. Slowly pressurize the vapor line while watching the gauge. The valve should open above 5.07 kPa (38 mmHg, 1.5 in.Hg).
   - If the pressure hold below 5.07 kPa (38 mmHg, 1.5 in.Hg), the valve is OK.
   - If the pressure doesn't hold, replace the EVAP two way valve.