( TL19E00K791000R461XFAAT00 )

DTC Troubleshooting: 46-1x

1. Measure the voltage between No. 1 terminal of SRS floor wire harness 2P connector and body ground, and between the No. 2 terminal and body ground. There should be less than 1.0 V.

Is the voltage as specified?

YES | - | Go to Step 13 .
NO | - | Short to power in the SRS floor wire harness; replace the SRS floor wire harness.■

1. Turn the ignition switch to LOCK (0).