( TL19E00J18573560321KBAT00 )

Trunk Lid Cylinder Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the body.

1. Remove these items:
   - Rear seat cushion
   - Rear seat side bolster, both sides
   - Rear door opening seal, as needed
   - Rear pillar trim, both sides
   - Rear center seat belt lower anchor
   - Rear shelf

1. Detach the trunk lid opener cable (A) from the key cylinder bracket (B), and disconnect the cable from the cable fastener (C). Take care not to kink the cable.
   NOTE: Check if the cable fastener is damaged or stress-whitened.