( TL19E1PE10410654801KBAT00 )

A/T Shift Solenoid Valve and Shift Solenoid Wire Harness Replacement

1. Remove the shift solenoid valve mounting bolts (F), then hold the shift solenoid valve body and remove the shift solenoid valves.
   NOTE: Do not hold the shift solenoid valve connector to remove the shift solenoid valve.

1. Install new O-rings (two O-rings per shift solenoid valve) (G) on the shift solenoid valve.
   NOTE: A new shift solenoid valve comes with new O-rings. If you install a new shift solenoid valve, use the O-rings provided with it.

1. Install shift solenoid valve C (brown connector), shift solenoid valve D (black connector), and shift solenoid valve E (black connector) by holding the shift solenoid valve body; make sure the mounting bracket contacts the servo body.
   Secure the shift solenoid valve C with the bolt.
   NOTE: Do not hold the shift solenoid valve connector to install the shift solenoid valve. Be sure to hold the shift solenoid valve body.

1. Install shift solenoid valve B (brown connector) by holding the shift solenoid valve body; make sure the mounting bracket contacts the bracket of shift solenoid valve E.

1. Install shift solenoid valve A (brown connector) by holding the shift solenoid valve body; make sure the mounting bracket contacts the bracket of shift solenoid valve D.
   NOTE: Do not install shift solenoid valves A and B before installing shift solenoid valves D and E. If shift solenoid valves A and B are installed before installing shift solenoid valves D and E, it may damage the hydraulic control system.

1. Secure shift solenoid valves B and E with the bolt, then secure shift solenoid valves A and D with the bolt.

1. Connect the shift solenoid wire harness terminals to shift solenoid valves:
   - BLU wire connector to shift solenoid valve A.
   - ORN wire connector to shift solenoid valve B.
   - GRN wire connector to shift solenoid valve C.
   - YEL, WHT, and WHT wire connector to shift solenoid valve D.
   - RED wire connector to shift solenoid valve E.

1. Install a new gasket, the dowel pins, and the shift solenoid valve cover.

1. Install a new O-ring on the ATF dipstick guide tube, then install the guide tube. Secure the guide tube with the bolts.

1. Check the shift solenoid wire harness connector for rust, dirt, or oil, and clean if necessary, then connect the connector securely.

1. Secure the ATF cooler line with the bolts.

1. Install the harness clamps on the clamp brackets.

1. Install the battery base.

1. Install the air cleaner housing and the intake air duct.

1. Install the splash shield.

1. Install the left front wheel.

1. Do the battery installation procedure.
   NOTE: Do not the test-driving until Step 34 .

1. Refill the transmission with ATF.