( TL19E00J26216550671KDAT00 )

Center Console Refrigerator Valve Removal/Installation

With Rear Ventilation
NOTE:

- Take care not to scratch the console.
- When removing components, use the trim tools or equivalent.

1. Open the console armrest.

1. Using the appropriate trim tool, pry up on the upper edge of the center console refrigerator valve assembly (A) to release the upper hook (B). Release the lower hook (C), then remove the valve assembly.