( TL19E1AE34116317044KBAT00 )

Clutch Pedal Cover Replacement

NOTE: This procedure is for models equipped with a metal clutch pedal plate model.

1. Cover the carpet under the clutch pedal to prevent metal shavings from getting on the carpet.

1. Center-punch each of the rivets (A), and drill their heads off with a 3 mm (0.12 in.) drill bit (B).
   NOTE: Do not drill the clutch pedal pad (C).

1. Remove the clutch pedal plate (A) and the clutch pedal cover (B) from the clutch pedal pad (C).

1. Set the clutch pedal cover to the clutch pedal plate.

1. Install the clutch pedal plate (A) with the rivets (B) firmly.

1. Using your hand, make sure the clutch pedal cover is firmly fastened to the pedal.

1. Check the clutch pedal height.