( TL19E00B20200000000MBAT00 )

Wheel Alignment

Rear Toe Inspection/Adjustment

1. Release the parking brake to avoid and incorrect measurement.

1. Check the toe.

   Rear toe-in: | 2±2 mm (0.08±0.08 in.)

   - If adjustment is required, go to Step 3 .
   - If no adjustment is required, measure the turning angle.

1. Hold the adjusting bolt (A) on the rear control arm (B), and loosen the self-locking nut (C).

1. Replace the self-locking nut with a new one, and lightly tighten it.
   NOTE: Always use a new self-locking nut whenever it has been tightened to the specified torque.

1. Adjust the rear toe by turning the adjusting bolt until the toe is correct.

1. Tighten the self-locking nut while holding the adjusting bolt to the specified torque valve.