( TL19E00H46400055408KBAT00 )

Side Curtain Airbag Replacement

1. Connect the SRS floor wire harness 2P connectors (A) to the side curtain airbags.

1. Do the battery terminal reconnection procedure.

1. Connect the HDS, and clear the DTCs.

1. After installing the side curtain airbag, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off.

1. Install all removed parts.

1. Confirm proper headliner/pillar trim overlap.