( TL19E00J2620005729PKDAT00 )

Sunvisor Removal/Installation

1. If the side curtain airbag has not deployed, to prevent the side curtain airbags from deploying improperly and possibly causing injury, inspect removed sunvisor and replace it if it has any cracks or breakages:
   - Any cracks in the sunvisor bracket (A)
   - Any cracks in the sunvisor bracket cover (B)
   - Any bends or cracks in the sunvisor stay shaft (C)
   - Any cracks in the sunvisor base (D)
   - Any cracks in the vanity mirror base (E)

1. If the holder grommet is damaged or stress-whitened, replace it with a new one.