( TL19E00J10300000000CAAT10 )

Stereo Amplifier Connector for Inputs and Outputs
Premium Audio System
STEREO AMPLIFIER CONNECTOR A (18P)
Stereo Amplifier Connector A (18P)

Cavity | Wire | Connects to
--- | --- | ---
A1 | LT BLU | Subwoofer (SUBW SP−)
A2 | BLU | Front center speaker (CTR SP−)
A3 | BLU | Right rear door speaker (RR SP−)
A4 | GRN | Left rear door speaker (RL SP−)
A5 | ORN [BRN] | Right rear speaker (SAT R SP−)
A6 | GRN | Right front door speaker, right front door tweeter (FR SP−)
A7 | BLU | Left front door speaker, left front door tweeter (FL SP−)
A8 | BRN | Left rear speaker (SAT L SP−)
A9 | BLK | Ground (G601) (GND)
A10 | GRY | Subwoofer (SUBW SP+)
A11 | YEL | Front center speaker (CTR SP+)
A12 | RED | Right rear door speaker (RR SP+)
A13 | WHT | Left rear door speaker (RL SP+)
A14 | BLU [PNK] | Right rear speaker (SAT R SP+)
A15 | RED | Right front door speaker, right front door tweeter (FR SP+)
A16 | BLK | Left front door speaker, left front door tweeter (FL SP+)
A17 | YEL | Left rear speaker (SAT L SP+)
A18 | LT BLU | Constant power (+B)

[ ]: | RHD model

STEREO AMPLIFIER CONNECTOR B (28P)
Stereo Amplifier Connector B (28P)

Cavity | Wire | Connects to
--- | --- | ---
B1 | RED | Audio unit (ELS DATA−)
B2 | BLK | Ground (G401) (GND)
B3 | YEL | Audio unit (SWD +B)
B8 *1 | GRY *2 | Navigation unit (NAVI SH GND)
B9 *1 | WHT [BLK] | Navigation unit (NAVI GND)
B10 | BLK | Audio unit (FL PRE+)
B11 | GRN | Audio unit (FR PRE+)
B12 | GRY *2 | Audio unit (SH FR-FL GND)
B15 | GRN | Audio unit (ELS DATA+)
B16 | GRY *2 | Audio unit (SH ELS GND)
B21 *1 | BLK [WHT] | Navigation unit (NAVI LCH)
B24 | WHT | Audio unit (FL PRE−)
B25 | RED | Audio unit (FR PRE−)

*1: | With navigation system
*2: | The shielded wires have a heat-shrink tube insulating the outside of the wire. The color of the insulating tube, typically black or dark gray, may not match the color of the wire shown on the circuit diagram.

[ ]: | RHD model