( TL19E1PE10400000000HAAT15 )

Vehicle moves in D and R, but not in 2nd in S

Probable Cause(s)

1. 2nd accumulator defective
2. 2nd gears worn or damaged
3. 2nd clutch defective

Notes

- Check the 2nd clutch pressure.
- Inspect the clutch piston, the clutch piston check valve, and the O-rings. Check the spring retainer and the retainer seal for wear and damage. Inspect the clearance between the clutch end-plate and the top disc. If the clearance is out of tolerance, inspect the clutch discs and the plates for wear and damage. If the discs are worn or damaged, replace them as a set. Inspect the clutch wave-plate height. If the height is out of tolerance, replace the wave-plate. If the discs and the plates are OK, adjust the clearance with the clutch end-plate.