( TL19E00J10300027201FHAT00 )

Speaker Test/Replacement

Rear Speaker

1. Remove the speaker grille.

1. Remove the mounting bolt, then tilt the speaker forward to release the front clips (A).
   If you pull the speaker out too far from the rear bulkhead, you will damage the lower clips.

1. Disconnect the 2P connector (B), and remove the rear speaker.

1. Measure the resistance between the terminals No. 1 and No. 2. There should be about 4 Ω.

1. If the resistance is not as specified, replace the rear speaker.