( TL19E00J46643427905FHAT00 )

Fuel Fill Door Lock Actuator Test/Replacement

1. Open the trunk lid, and remove the left trunk side trim panel.

1. Disconnect the 2P connector (A) from the fuel fill door lock actuator (B).

1. Check actuator operation by connecting power to the No. 2 terminal and ground to the No. 1 connector momentarily.
   NOTE: To prevent damage to the solenoid apply battery voltage momentarily.

1. If the actuator does not operate, replace it.