( TL19E00J26220219365KDAT00 )

Dashboard Passenger's Trim Removal/Installation

NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Remove the passenger's dashboard trim (A).

   -1. | Open the glove box.
   -2. | Pull out on the bottom edge of the trim by hand.
   -3. | Detach the clips along the trim.

1. Install the trim in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.